#calibration_ok:[2:19:11] 



at version:release/V4.18_P2.29.2 sdk version:amebad_v6.2C firmware version:release/V4.18_P5.6.4(May 30 2023-10:28:28)


config not init
[AI_LoadConfigFromFlash()-668]load default config
[AI_LoadConfigFromFlash()-794]AI_HalBleGetMac ret=2 mac:000000000000
[AI_LoadConfigFromFlash()-808]skip iBeaconUUID init,wait ble mac init
[AI_HalWriteFlash()-328]flash save ok
[AI_LoadConfigFromFlash()-843]save config ret=0
[AI_ComboInit()-201]load config ret=2
[AI_ComboInit()-204]init AT uart ret=0
interface 0 is initialized
interface 1 is initialized

Initializing WIFI ...[AI_WatchdogThread()-626]AI_HalWatchdogRefresh start
[AI_WifiInitCallbak()-750]

WIFI initialized
[wifi_set_country_code()-656]not set country code

init_thread(58), Available heap 0x25ca0ble_common_init 0 

BT BUILD Date: 2023/05/30-10:27:41 
BT Reset...
salve_add_server 
GAP_INIT_STATE_STACK_READY 
physical efuse: has data hci_tp_phy_efuse[1]= 9e 

hci_tp_phy_efuse[0]=0,
bt_iqk_dump:    DUMP,
the IQK_xx  data is 0x10c,
the IQK_yy  data is 0x3fe,
the QDAC  data is 0x1e,
the IDAC  data is 0x20,
hci_read_rom_check: rom_version 0x0002, bt_hci_chip_id 0x0003
BT ADDRESS: 94:c9:60:01:cd:1e

 WRITE  physical FLATK=tx_flatk=1 

hci_tp_config:BT INIT success 7
Start upperStack
app_handle_gap_msg: subtype 1
salve_handle_dev_state_evt: init state 1, adv state 0, cause 0x0
[BLE peripheral] GAP stack ready
app_handle_gap_msg: subtype 1
salve_handle_dev_state_evt: init state 1, adv state 1, cause 0x0app_handle_gap_msg: subtype 1
salve_handle_dev_state_evt: init state 1, adv state 2, cause 0x0
GAP adv start
ble_common_init success 
[RTL_HalBleMacInit()-304]start ble success
[RTL_HalBleMacInit()-320]BLE MAC init:94c96001cd1e
[BLE Peripheral]BT Stack deinitalized
[RTL_HalBleMacInit()-326]stop ble success
[AI_ProcessThread()-1022]init iBeaconUUID and slave adv BleMac
ble_common_init 0 

BT BUILD Date: 2023/05/30-10:27:41 
BT Reset...
salve_add_server 
GAP_INIT_STATE_STACK_READY 
physical efuse: has data hci_tp_phy_efuse[1]= 9e 

hci_tp_phy_efuse[0]=0,
bt_iqk_dump:    DUMP,
the IQK_xx  data is 0x10c,
the IQK_yy  data is 0x3fe,
the QDAC  data is 0x1e,
the IDAC  data is 0x20,
hci_read_rom_check: rom_version 0x0002, bt_hci_chip_id 0x0003
BT ADDRESS: 94:c9:60:01:cd:1e

 WRITE  physical FLATK=tx_flatk=1 

hci_tp_config:BT INIT success 7
Start upperStack
app_handle_gap_msg: subtype 1
salve_handle_dev_state_evt: init state 1, adv state 0, cause 0x0
[BLE peripheral] GAP stack ready
app_handle_gap_msg: subtype 1
salve_handle_dev_state_evt: init state 1, adv state 1, cause 0x0app_handle_gap_msg: subtype 1
salve_handle_dev_state_evt: init state 1, adv state 2, cause 0x0
GAP adv start
ble_common_init success 
[AI_HalWriteFlash()-328]flash save ok
[AI_AutoConnectOnboot()-946]wifi auto connect off
[AI_AutoConnectOnboot()-1003]ble auto connect off
