ESP8266_RTOS_SDK v1.4.0

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
station_config Struct Reference
WiFi Related APIs » Station APIs

## Data Fields
uint8 | ssid [32]
uint8 | password [64]
uint8 | bssid_set
uint8 | bssid [6]

## Field Documentation

uint8 bssid[6]

MAC address of target AP

uint8 bssid_set

whether set MAC address of target AP or not. Generally, station_config.bssid_set needs to be 0; and it needs to be 1 only when users need to check the MAC address of the AP.

uint8 password[64]

password of target AP

uint8 ssid[32]

SSID of target AP

The documentation for this struct was generated from the following file:

- include/espressif/esp_sta.h