ESP8266_RTOS_SDK v1.4.0

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
Event_SoftAPMode_StaDisconnected_t Struct Reference
WiFi Related APIs » Common APIs

## Data Fields
uint8 | mac [6]
uint8 | aid

## Field Documentation

uint8 aid

the aid that ESP8266 soft-AP gave to the station disconnects to

uint8 mac[6]

MAC address of the station disconnects to ESP8266 soft-AP

The documentation for this struct was generated from the following file:

- include/espressif/esp_wifi.h