ESP8266_RTOS_SDK v1.4.0

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
Event_StaMode_AuthMode_Change_t Struct Reference
WiFi Related APIs » Common APIs

## Data Fields
uint8 | old_mode
uint8 | new_mode

## Field Documentation

uint8 new_mode

the new auth mode of AP

uint8 old_mode

the old auth mode of AP

The documentation for this struct was generated from the following file:

- include/espressif/esp_wifi.h