ESP8266_RTOS_SDK v1.4.0

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
_esp_tcp Struct Reference
Network Espconn APIs

## Data Fields
int | remote_port
int | local_port
uint8 | local_ip [4]
uint8 | remote_ip [4]
espconn_connect_callback | connect_callback
espconn_reconnect_callback | reconnect_callback
espconn_connect_callback | disconnect_callback
espconn_connect_callback | write_finish_fn

## Field Documentation

espconn_connect_callback connect_callback

connected callback

espconn_connect_callback disconnect_callback

disconnected callback

uint8 local_ip[4]

local IP of ESP8266

int local_port

ESP8266's local port of TCP connection

espconn_reconnect_callback reconnect_callback

as error handler, the TCP connection broke unexpectedly

uint8 remote_ip[4]

remote IP of TCP connection

int remote_port

remote port of TCP connection

espconn_connect_callback write_finish_fn

data send by espconn_send has wrote into buffer waiting for sending, or has sent successfully

The documentation for this struct was generated from the following file:

- include/espressif/espconn.h