ESP8266_RTOS_SDK v1.4.0

- Main Page
- Modules
- Data Structures
- Files

- File List

esp_spiffs.h
1 /*
2 * ESPRSSIF MIT License
3 *
4 * Copyright (c) 2015 <ESPRESSIF SYSTEMS (SHANGHAI) PTE LTD>
5 *
6 * Permission is hereby granted for use on ESPRESSIF SYSTEMS ESP8266 only, in which case,
7 * it is free of charge, to any person obtaining a copy of this software and associated
8 * documentation files (the "Software"), to deal in the Software without restriction, including
9 * without limitation the rights to use, copy, modify, merge, publish, distribute, sublicense,
10 * and/or sell copies of the Software, and to permit persons to whom the Software is furnished
11 * to do so, subject to the following conditions:
12 *
13 * The above copyright notice and this permission notice shall be included in all copies or
14 * substantial portions of the Software.
15 *
16 * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 * IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS
18 * FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR
19 * COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER
20 * IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN
21 * CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
22 *
23 */
24
25 #ifndef __ESP_SPIFFS_H__
26 #define __ESP_SPIFFS_H__
27
28 #include "spiffs/spiffs.h"
29
30 #ifdef __cplusplus
31 extern "C" {
32 #endif
33
45 struct esp_spiffs_config {
46 uint32 phys_size;
47 uint32 phys_addr;
48 uint32 phys_erase_block;
50 uint32 log_block_size;
51 uint32 log_page_size;
53 uint32 fd_buf_size;
54 uint32 cache_buf_size;
55 };
56
65 sint32 esp_spiffs_init(struct esp_spiffs_config *config);
66
74 void esp_spiffs_deinit(uint8 format);
75
80 #ifdef __cplusplus
81 }
82 #endif
83
84 #endif /* __ESP_SPIFFS_H__ */
esp_spiffs_config::phys_addr
uint32 phys_addr
Definition: esp_spiffs.h:47
esp_spiffs_init
sint32 esp_spiffs_init(struct esp_spiffs_config *config)
Initialize spiffs.
esp_spiffs_config::log_block_size
uint32 log_block_size
Definition: esp_spiffs.h:50
esp_spiffs_config::phys_erase_block
uint32 phys_erase_block
Definition: esp_spiffs.h:48
esp_spiffs_config::fd_buf_size
uint32 fd_buf_size
Definition: esp_spiffs.h:53
esp_spiffs_deinit
void esp_spiffs_deinit(uint8 format)
Deinitialize spiffs.
esp_spiffs_config::cache_buf_size
uint32 cache_buf_size
Definition: esp_spiffs.h:54
esp_spiffs_config::log_page_size
uint32 log_page_size
Definition: esp_spiffs.h:51
esp_spiffs_config::phys_size
uint32 phys_size
Definition: esp_spiffs.h:46
esp_spiffs_config
Definition: esp_spiffs.h:45